        Realtek Semiconductor Corp. High-Speed USB Media Card Reader Software Ver:1.0.0.0
                        Installation and Setup


Driver Installation/Removal Procedure For High-Speed USB Media Card Reader:
=================================================================================

<<< For Windows Vista x86/x64 (WDM driver) >>>

---------------------------------------
Setup Driver at first time:
---------------------------------------

Step 1. Before installing the Realtek High-Speed USB Media Card Reader Drivers, Press the
        [Cancel] button if Windows detect the USB Card Reader device. 
          
Step 2. Insert the "Realtek High-Speed USB Media Card Reader Drivers" CD into the CD-ROM 
        drive and run the setup.exe program to finish the installation. 

Step 3. Click on [Next/OK/Go] to continue the procedure. If the Windows popup 
        "Digital Signature Not Found" message, press [Yes] to continue the 
        installation.
        
Step 4. Finally, select to restart the system and press [Finish] to complete
        the installation.  

        The system will reload the drivers and do some adjustments in the INF
        file if so required.

--------------------------
Update Driver:
--------------------------

Step 1. Follow Step 2,3,4 described in [Setup at first time] above to complete
        the procedure.

--------------------------
Remove Driver:
--------------------------

Step 1. Go to Start\Settings\Control Panel.

Step 2. Select [Add/Remove Programs] icon.

Step 3. Select "Realtek USB 2.0 Card Reader" and press [Change/Remove]
        button.

Step 4. Click on [Next/OK/Go] to finish the uninstallation.        

Step 5. At the end of the procedure, select to restart the system and press
        [Finish] to complete the uninstallation.



<< Other Informations >>

--------------------
Silent Installation:
--------------------

Run "Setup.exe /s /f2<path\LogFile> /z[-rp<path\LogFile>]"
i.e. setup.exe /s /f2c:\mylog.log /z[-rpC:\RTCRSetup.log]

--------------------
Silent Uninstallation:
--------------------

Run "Setup.exe /removeonly /s /f1<path\Setup.iss> /f2<path\LogFile> /z[-rp<path\LogFile>]"
i.e. setup.exe /removeonly /s /f1C:\CRDriver\Setup.iss /f2c:\mylog.log /z[-rpC:\RTCRSetup.log]

---------------------
Version Informations:
---------------------
If driver package include below drivers :
Vista driver : --------------------------------------------------------
Vista driver for x86
RTSTOR.sys                                         : 6.0.6000.20097
DriveIcon.dll                                      

Vista driver for x64
RTSTOR64.sys                                       : 6.0.6000.20097
DriveIcon.dll                                          