======================================================================================================
Date 		: 2007/05/10/17:33
Driver Name	: BisonCamInstall-D(0705101733)-V(6.32.64.703.2)_clevo_uvc1300_vista3264_test
Versiion	: 6.32.64.703.2
note		: 
=======================================================================================================
Date 		: 2007/05/16/17:55
Driver Name	: BisonCamInstall-D(0705161755)-V(6.32.64.703.2)_clevo_uvc1300_vista3264_test
Versiion	: 6.32.64.703.2
note		: fix ap action and error message
=======================================================================================================
Date 		: 2007/05/18/15:51
Driver Name	: BisonCamInstall-D(0705181551)-V(6.32.64.703.2)_clevo_uvc1300_vista3264_test
Versiion	: 6.32.64.703.2
note		: fix can't preview
=======================================================================================================
Date 		: 2007/05/24/14:38
Driver Name	: BisonCamInstall-D(0705241438)-V(6.32.64.703.2)_clevo_uvc1300_vista3264_test
Versiion	: 6.32.64.703.2
note		: 
=======================================================================================================
Date 		: 2007/06/07/18:42
Driver Name	: BisonCamInstall-D(0706071842)-V(6.32.64.703.2)_clevo_uvc1300_vista3264_test
Versiion	: 6.32.64.703.2
note		: 
=======================================================================================================
Date 		: 2007/06/12/18:00
Driver Name	: BisonCamInstall-D(0706121800)-V(6.32.64.703.2)_clevo_uvc1300_vista3264_test
Versiion	: 6.32.64.703.2
note		: 
=======================================================================================================
Date 		: 2007/06/21/11:43
Driver Name	: BisonCamInstall-D(0706211143)-V(6.32.64.703.2)_clevo_uvc_common_vista3264_test
Versiion	: 6.96.704.2
note		: 
=======================================================================================================
Date 		: 2007/06/22/18:54
Driver Name	: BisonCamInstall-D(0706221854)-V(6.96.704.2)_clevo_uvc_common_vista3264_test
Versiion	: 6.96.704.2
note		: 
=======================================================================================================
Date 		: 2007/06/23/11:51
Driver Name	: BisonCamInstall-D(0706231151)-V(6.96.704.2)_clevo_uvc_common_vista3264_test
Versiion	: 6.96.704.2
note		: 
=======================================================================================================
Date 		: 2007/06/26/17:46
Driver Name	: BisonCamInstall-D(0706261746)-V(6.96.704.2)_clevo_uvc_common_vista3264_test
Versiion	: 6.96.704.2
note		: fix uac and add size 1680x1050
=======================================================================================================
Date 		: 2007/06/29/14:01
Driver Name	: BisonCamInstall-D(0706291401)-V(6.96.704.2)_clevo_uvc_common_vista3264_test
Versiion	: 6.96.704.2
note		: fix uac 
=======================================================================================================
Date 		: 2007/07/04/15:56
Driver Name	: BisonCamInstall-D(0707041556)-V(6.96.704.2)_clevo_uvc_common_vista3264_whql
Versiion	: 6.96.704.2
note		: pass WHQL
=======================================================================================================
Date 		: 2007/07/11/16:41
Driver Name	: BisonCamInstall-D(0707111641)-V(6.96.704.2.1)_clevo_uvc_common_vista3264_whql
Versiion	: 6.96.704.2.1
note		: ap will close when into s3s4 from clevo's request ;fix 2m snap issue with format 1680x1050
=======================================================================================================
Date 		: 2007/07/13/11:02
Driver Name	: BisonCamInstall-D(0707131102)-V(6.96.704.2.3)_clevo_uvc_common_vista3264_whql
Versiion	: 6.96.704.2.3
note		: make ap can only open once
=======================================================================================================
Date 		: 2007/07/25/19:32
Driver Name	: BisonCamInstall-D(0707251932)-V(6.96.704.2.5)_clevo_uvc_common_vista3264_whql
Versiion	: 6.96.704.2.5
note		: fix s3 white screen & find new hardware issue 
=======================================================================================================
Date 		: 2007/07/27/20:01
Driver Name	: BisonCamInstall-D(0707272001)-V(6.96.704.2.7)_clevo_uvc_common_vista3264_whql
Versiion	: 6.96.704.2.7
note		: fix preview lag when dc mode
=======================================================================================================
Date 		: 2007/07/30/20:54
Driver Name	: BisonCamInstall-D(0707302054)-V(6.96.704.2.9)_clevo_uvc_common_vista3264_whql
Versiion	: 6.96.704.2.9
note		: fix platform will hang up when into s3 on xp
=======================================================================================================
BisonCamInstall-D(0708252244)-V(6.96.704.2.11)_clevo_uvc_common_vista3264_close_ap
Date 		: 2007/08/25/22:44
Versiion	: 6.96.704.2.11
note		: Update system file for 4AA+5607 & 4B1+5607
		  For 4AA+5607, this driver should used on non VIA NB.
		  For 4B1+5607, this driver can fix preview issue by change format to YUY2.
		  XP 32 bit support CPU sleep status.
=======================================================================================================
BisonCamInstall-D(0708252250)-V(6.96.704.2.13)_clevo_uvc_common_vista3264_VIA_close_ap
Date 		: 2007/08/25/22:50
Versiion	: 6.96.704.2.13
note		: Update system file for 4AA+5607 & 4B1+5607.
		  For 4AA+5607, this driver should used on VIA NB.
		  And it can fix preview lag issue on VIA NB & jumping blue piexl issue if background is black.
		  For 4B1+5607, this driver can fix preview issue by change format to YUY2.
		  XP 32 bit support CPU sleep status.
=======================================================================================================
BisonCamInstall-D(0708291701)-V(6.96.704.2.15)_clevo_uvc_common_vista3264_close_ap
Date 		: 2007/08/29/17:01
Versiion	: 6.96.704.2.15
note		: To fix driver install issue on Vista 64, we add one lose file bisonr67.dll.
=======================================================================================================
BisonCamInstall-D(0708312149)-V(6.96.704.2.17)_clevo_uvc_common_vista3264_close_ap
Date 		: 2007/08/31/21:49
Versiion	: 6.96.704.2.17
note		: Update system file to fix capture issue.
=======================================================================================================
BisonCamInstall-D(0708312159)-V(6.96.704.2.19)_clevo_uvc_common_vista3264_VIA_close_ap
Date 		: 2007/08/31/21:59
Versiion	: 6.96.704.2.19
note		: Update system file to fix capture issue.
=======================================================================================================
BisonCamInstall-D(0709062219)-V(6.96.704.2.21)_clevo_uvc_common_vista3264_close_ap
Date 		: 2007/09/06/22:19
Versiion	: 6.96.704.2.21
note		: Update system file for 4AA+5607 to fix cross line issue.
=======================================================================================================
BisonCamInstall-D(0709072159)-V(6.96.704.2.23)_clevo_uvc_common_vista3264_VIA_close_ap
Date 		: 2007/09/07/21:59
Versiion	: 6.96.704.2.23
note		: Update system file with new link for 4AA+5607 to fix cross line issue by check package.
=======================================================================================================
BisonCamInstall-D(0709102219)-V(6.96.704.2.25)_clevo_uvc_common_vista3264_close_ap
Date 		: 2007/09/10/22:19
Versiion	: 6.96.704.2.25
note		: Update system file for PT80V(UMPC) with 20 fps setting in VGA.
		  Off RGB24 format for PT80V(UMPC).
=======================================================================================================
BisonCamInstall-D(0709102226)-V(6.96.704.2.27)_clevo_uvc_common_vista3264_VIA_close_ap
Date 		: 2007/09/10/22:26
Versiion	: 6.96.704.2.27
note		: Update system file for PT80V(UMPC) with 20 fps setting in VGA.
		  Off RGB24 format for PT80V(UMPC).
=======================================================================================================
BisonCamInstall-D(0709112023)-V(6.96.704.2.29)_clevo_uvc_common_vista3264_PT80V_close_ap
Date 		: 2007/09/11/20:23
Versiion	: 6.96.704.2.29
note		: Update image size for PT80V.
		  Add I420 format for PT80V.
		  Update preview application without Zomm function.
=======================================================================================================
BisonCamInstall-D(0709122127)-V(6.96.704.2.23)_clevo_uvc_common_vista3264_VIA_close_ap_WHQL
Date 		: 2007/09/12/21:27
Versiion	: 6.96.704.2.23
note		: Get WHQL for 4AA+5607.
		  Use RGB24 as default format by change preview setting.
=======================================================================================================
BisonCamInstall-D(0709131045)-V(6.96.704.2.29)_clevo_uvc_common_vista3264_PT80V_close_ap_WHQL
Date 		: 2007/09/13/10:45
Versiion	: 6.96.704.2.29
note		: Get logo for 6.96.704.2.29.
=======================================================================================================
BisonCamInstall-D(0709142354)-V(6.96.704.3.1)_clevo_uvc_common_vista3264_WHQL_close_ap
Date 		: 2007/09/14/23:54
Versiion	: 6.96.704.3.1
Project		: D900C/M570RU	(NON-VIA	RGB24 as default	AP auto close while S3/S4)
note		: Get logo for 6.96.704.2.21.
		  Update preview application without "Save Capture Video as" & TIME LIMIT.
=======================================================================================================
BisonCamInstall-D(0709291212)-V(6.96.704.3.9)_clevo_uvc_common_vista3264
Date 		: 2007/09/29/12:12
Versiion	: 6.96.704.3.9
Project		: D900C/M570RU	(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU	(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 	(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 	(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
note		: Update new TSR for snapshot function(cannot take a picture after long time burning test).
		  Update 2M driver with shorter waiting time before into selective suspend.
		  Fix install driver issue after plug-in device in Vista Home Basic 32 bit OS.
		  Add multi-language in user interface.
		  Update OEM.ini with new function : [Preview]
						     ZoomIn_Out=yes			yes  : preview application with zoom in/zoom out function.
											no   : preview application without zoom in/zoom out function.
						     Close_AP_BeforeSleep=no		yes  : preview application will auto close before into S3/S4.
											no   : preview application won't auto close before into S3/S4.
						     DefaultFormat_YUY2_RGB24=yuy2	yuy2 : preview application will use YUY2 as default format.
											rgb24: preview application will use RGB24 as default format.

						     [PowerSaving]
						     SelectiveSuspend=yes		yes  : support selective suspend.
											no   : not support selective suspend.
=======================================================================================================
BisonCamInstall-D(0710031150)-V(6.96.704.3.12)_clevo_uvc
Date 		: 2007/10/03/11:50
Versiion	: 6.96.704.3.12
Project		: D900C/M570RU	(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU	(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 	(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 	(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
note		: Update new TSR for snapshot function(cannot take a picture after install TV Tuner's driver).
		  Fix error message after finish installation.
		  Fix OEM.ini function : DefaultFormat_YUY2_RGB24.
=======================================================================================================
BisonCamInstall-D(0710252247)-V(6.96.704.3.15)_clevo_uvc
Date 		: 2007/10/25/22:47
Versiion	: 6.96.704.3.15
Project		: D900C/M570RU	(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU	(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 	(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 	(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
note		: Update new TSR for c3 issue.
		  Fix install issue if plug in device after install driver.
=======================================================================================================
BisonCamInstall-D(0711051703)-V(6.96.704.3.16)_clevo_uvc
Date 		: 2007/11/05/17:03
Versiion	: 6.96.704.3.16
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Update 32/64 bit driver with newest link to fix S3/S4 & Fn+F10 blue screen issue & blurred screen issue & DTM test issue.
		  Update new preview application to fix black or white screen issue.
		  Update TSR for Zoom in/out display string issue.
		  Combin non-VIA & VIA & PT80V in same driver by change flag in OEM.ini : 
			[Module]
			1.3M_OR_2M=1.3m		//set 2M if camera module is 2M

			[Platform]
			Is_VIA=no		//set yes if platform is VIA
			Is_PT80V=no		//set yes if platform is PT80V
=======================================================================================================
BisonCamInstall-D(0711141742)-V(6.96.704.3.17)_clevo_uvc
Date 		: 2007/11/14/17:42
Versiion	: 6.96.704.3.17
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Update new preview application to fix write screen issue before move mouse.
		  Del "1.3M_OR_2M" in OEM.ini and auto detect 1.3M or 2M.
=======================================================================================================
BisonCamInstall-D(0711262152)-V(6.96.704.4.1)_clevo_uvc_WHQL
Date 		: 2007/11/26/21:52
Versiion	: 6.96.704.4.1
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Get logo from 6.96.704.3.17.
=======================================================================================================
BisonCamInstall-D(0711271851)-V(6.96.704.4.2)_clevo_uvc_WHQL
Date 		: 2007/11/27/18:51
Versiion	: 6.96.704.4.2
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Add manifest on exe file which is used to install camera driver after plug-in device.
=======================================================================================================
BisonCamInstall-D(0711301918)-V(6.96.704.4.3)_clevo_uvc_WHQL
Date 		: 2007/11/30/19:18
Versiion	: 6.96.704.4.3
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Update preview application with retry 5 sec setting.
=======================================================================================================
BisonCamInstall-D(0712061430)-V(6.96.704.4.4)_clevo_uvc_WHQL
Date 		: 2007/12/06/14:30
Versiion	: 6.96.704.4.4
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Update "BisonHK.exe" to fix auto close issue.
		  Update preview application retry 5 sec after power off device.
=======================================================================================================
BisonCamInstall-D(0712062323)-V(6.96.704.4.5)_clevo_uvc_WHQL
Date 		: 2007/12/06/23:23
Versiion	: 6.96.704.4.5
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Add new PowerSaving flag : Powerdown, to open powerdownwhenunopen powersaving function.
=======================================================================================================
BisonCamInstall-D(0712072138)-V(6.96.704.4.6)_clevo_uvc_WHQL
Date 		: 2007/12/07/21:38
Versiion	: 6.96.704.4.6
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Update BisonHK.exe for take picture & zoom function.
		  Update preview application to show error message in 1 sec after press Fn+F10 during previewing.
=======================================================================================================
BisonCamInstall-D(0712081719)-V(6.96.704.4.7)_clevo_uvc_WHQL
Date 		: 2007/12/08/17:19
Versiion	: 6.96.704.4.7
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Update preview application to shorten the ap preview image time.
		  Update preview application to show error message in 1 sec after press Fn+F10 during previewing.
=======================================================================================================
BisonCamInstall-D(0712111512)-V(6.96.704.4.8)_clevo_uvc_WHQL
Date 		: 2007/12/11/15:12
Versiion	: 6.96.704.4.8
Project		: D900C/M570RU		(NON-VIA	RGB24 as default	AP auto close while S3/S4)
		  D900C/M570RU		(NON-VIA	RGB24 as default	AP won't auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP auto close while S3/S4)
		  M72S/R/M54JE 		(NON-VIA	YUY2 as default 	AP won't auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP auto close while S3/S4)
		  M54SE/M66SE/M67SI 	(VIA		YUY2 as default 	AP won't auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP auto close while S3/S4)
		  TP80V 		(VIA		YUY2 as default 	AP won't auto close while S3/S4)

note		: Auto reboot after install & uninstall.
=======================================================================================================
